This package contains the source code of the UWB ranging demo using ISP1510 Demo.

To open the project Keil µVison 5 is required.
The Nordic's s132_nrf52_3.1.0_softdevice is needed.

To generate an Anchor firmware, CONFIG_AS_ANCHOR symbol must be defined.
To generate a Tag firmware, CONFIG_AS_TAG symbol must be defined.
It can be defined in Project -> Options for target -> C/C++ -> Define